BASICFREQCD= 100
BASICFREQUD= 100
BASICFREQLIST= 100
BASICRATECD= 180
BASICRATEUD= 180
BASICRATELIST= 313,268,234,203,179,160,144,132,119,109,99,89,82,74,steady,off
HELPBASICL1= F1 toggles Freq. F2 steps through rates.
HELPBASICL2= Knob adjusts output current.
CS4FREQCD= 60
CS4FREQUD= 60
CS4FREQLIST= 100
CS4RATECD= 180
CS4RATEUD= 180
CS4RATELIST= 180,off,steady,75,120
CS4AMPSCD= 0.100
CS4AMPSUD= 0.100
CS4AMPSLIST= 0.100,0.200,0.300,0.400,0.500,0.600,0.700,0.800,0.900,1.000,1.500,2.000,2.500,3.000,4.000
CS4DUTYCD= 55
CS4DUTYUD= 55
CS4DUTYLIST= 40,45,50,55,60
HELPCS4L1= F1-F5 to select parameter. 2nd press to
HELPCS4L2= enable knob. Up-Dn scrolls stored value.
CS9FREQ1CD= 100
CS9FREQ1UD= 100
CS9FREQ1LIST= 100
CS9FREQ2CD= 100
CS9FREQ2UD= 100
CS9FREQ2LIST= 0,250
CS9RATECD= 420
CS9RATEUD= 420
CS9RATELIST= 420,off,steady,50,75,120,180,220,270
CS9AMPSCD= 0.100
CS9AMPSUD= 0.100
CS9AMPSLIST= 0.100,0.200,0.300,0.400,0.500,0.600,0.700,0.800,0.900,1.000,1.500,2.000,2.500,3.000,4.000
CS9DUTYCD= 45
CS9DUTYUD= 45
CS9DUTYLIST= 40,45,50,55,60
HELPCS9L1= F1-F5 to select parameter. F1 toggles
HELPCS9L2= Freq1 & Freq2. Up/Dn scrolls stored val.
HELPCS9FREQL1= F1,F2 value Freq1, F4,F5 value Freq2.
SPEED1ENCD= 0
SPEED1ENUD= 0
SPEED1VOLTSCD= 5.0
SPEED1VOLTSUD= 5.0
DIAMINCH1CD= 31
DIAMINCH1UD= 31
DIAMINCH1LIST= 30,31,32
DIAMCM1CD= 78.74
DIAMCM1UD= 78.74
DIAMCM1LIST= 76.2,78.74,81.28
PPREV1CD= 100
PPREV1UD= 100
PPREV1LIST= 1,10,100
SPEEDMODECD= 0
SPEEDMODEUD= 0
USEMETRICCD= 0
USEMETRICUD= 0
SPEED2ENCD= 0
SPEED2ENUD= 0
SPEED2VOLTSCD= 5.5
SPEED2VOLTSUD= 5.5
DIAMINCH2CD= 31
DIAMINCH2UD= 31
DIAMINCH2LIST= 30,31,32
DIAMCM2CD= 78.74
DIAMCM2UD= 78.74
DIAMCM2LIST= 76.2,78.74,81.28
PPREV2CD= 100
PPREV2UD= 100
PPREV2LIST= 1,10,100
HELPSPEEDL1= F1-turn speed on, F2-turn speed off.
HELPSPEEDL2= F3 and F4-set output frequency or speed
HELPSPEEDL3= depending on mode of operation.
HELPSPEEDL4= F5-setup speed outputs and mode.
HELPSPEEDSET1L1= F1-setup output 1, F2-setup output 2.
HELPSPEEDSET1L2= F3-set outputs to independent or slaved.
HELPSPEEDSET1L3= F4-set units to frequency, MPH or KPH.
HELPSPEEDSET1L4= DFLT-allows user to save or restore
HELPSPEEDSET1L5= slave/indep mode and units of measure.
HELPSPEEDSET2L1= F1, F2-controls selected output.
HELPSPEEDSET2L2= F3-sets voltage of selected output.
HELPSPEEDSET2L3= F4-sets pulses/rev. of selected output.
HELPSPEEDSET2L4= F5-sets wheel diam. for selected output.
HELPSPEEDSET2L5= DFLT-allows user to save or restore
HELPSPEEDSET2L6= enable, voltage, pulses/rev and diam.
HELPMAINL1= Press F1-F5 to select operating mode.
HELPPARAML1= F1-F5 to select value. 2nd press to
HELPPARAML2= enable knob. Up-Dn scrolls stored value.
PASSCODE= 12345
USECODE= 1
HELPDFLTP1L1= F1 to save current values as defaults.
HELPDFLTP1L2= F5 to cancel save. Page for next choice.
HELPDFLTP2L1= F1 to restore user defaults.
HELPDFLTP2L2= F5 to cancel. Page for next choice.
HELPDFLTP3L1= F1 to restore customer defaults.
HELPDFLTP3L2= F5 to cancel save. Page for next choice.
HELPDFLTP4L1= F1 to restore factory defaults.
HELPDFLTP4L2= F5 to cancel save. Page for next choice.
HELPRAMPL1= F1-Start Value, F3-Stop Value, F5 time.
HELPRAMPL2= Up/Dn,Knob,adjust, start to run & save.
HELPDVML1= F1 turns off DVM, F2 for Ac, F3 for DC.
